server-identifier dhcp01.phx2.fedoraproject.org;                   
ddns-update-style none;                                         

subnet 10.5.125.0 netmask 255.255.255.0 {
    allow booting;                       
    allow bootp;                         

    option domain-name "phx2.fedoraproject.org";
    option domain-name-servers 10.5.126.21, 10.5.126.22;          
    option routers 10.5.125.254;                                  
#    option vendor-class-identifier "PXEClient";                  
#    option vendor-encapsulated-options 09:0f:80:00:0c:4e:65:74:77:6f:72:6b:20:62:6f:6f:74:0a:07:00:50:72:6f:6d:70:74:06:01:02:08:03:80:00:00:47:04:80:00:00:00:ff;


    host unknown00 {
        hardware ethernet 00:21:5e:5b:19:96;
	fixed-address 10.5.125.33;
        next-server 10.5.125.43;
        option host-name "unknown00.phx2.fedoraproject.org";
#        filename "yaboot";
    }    

    host sign-vault03 {
         hardware ethernet fc:99:47:49:43:84;
         fixed-address 10.5.125.73;
         option host-name "sign-vault03";
	 next-server 10.5.126.41;
	 filename "pxelinux.0";
    }

    host sign-vault04 {
         hardware ethernet fc:99:47:49:8d:fc;
         fixed-address 10.5.125.74;
         option host-name "sign-vault04";
	 next-server 10.5.126.41;
	 filename "pxelinux.0";
    }

    host bkernel01 {
    	 hardware ethernet 6c:ae:8b:1e:fd:82;
         fixed-address 10.5.125.51;
         option host-name "bkernel01";
	 next-server 10.5.126.41;
	 filename "pxelinux.0";
    }

    host bkernel02 {
    	 hardware ethernet 6c:ae:8b:1e:fd:6a;
         fixed-address 10.5.125.52;
         option host-name "bkernel02";
	 next-server 10.5.126.41;
	 filename "pxelinux.0";
    }

    host sign-vault01 {
        hardware ethernet 00:1a:64:67:a3:38;
        fixed-address 10.5.125.70;
	next-server 10.5.126.41;
        option host-name "sign-vault01";
	filename "pxelinux.0";
    }

    host bvirthost01 {
        hardware ethernet e4:1f:13:6a:c5:58;
        fixed-address 10.5.125.124;
        next-server 10.5.125.43;
        option host-name "bvirthost01";
	filename "pxelinux.0";
    }

    host bvirthost04 {
        hardware ethernet E4:1F:13:BA:E8:28;
        fixed-address 10.5.125.127;
        next-server 10.5.125.43;
        option host-name "bvirthost04";
	filename "pxelinux.0";
    }

    host bvirthost06 {
        hardware ethernet 00:25:B5:FF:00:09;
        fixed-address 10.5.125.120;
        next-server 10.5.126.41;
        option host-name "bvirthost06";
	filename "pxelinux.0";
    }

    host bvirthost07 {
        hardware ethernet 90:B1:1C:32:7E:8E;
        fixed-address 10.5.125.122;
	next-server 10.5.126.41;
        option host-name "bvirthost07";
	filename "pxelinux.0";
    }

    host bvirthost08 {
        hardware ethernet 00:25:B5:FF:00:07;
        fixed-address 10.5.125.123;
        next-server 10.5.126.41;
        option host-name "bvirthost08";
	filename "pxelinux.0";
    }

    host bvirthost09 {
        hardware ethernet 00:25:B5:FF:00:0F;
        fixed-address 10.5.125.117;
        next-server 10.5.126.41;
        option host-name "bvirthost09";
	filename "pxelinux.0";
    }

    host bvirthost10 {
        hardware ethernet 00:25:B5:FF:00:0D;
        fixed-address 10.5.125.118;
        next-server 10.5.126.41;
        option host-name "bvirthost10";
	filename "pxelinux.0";
    }

    host bvirthost11 {
        hardware ethernet 00:25:B5:FF:00:0B;
        fixed-address 10.5.125.119;
        next-server 10.5.126.41;
        option host-name "bvirthost11";
	filename "pxelinux.0";
    }


    host buildvmhost-10 {
        hardware ethernet 00:25:B5:FF:00:03;
        fixed-address 10.5.125.132;
	next-server 10.5.125.43;
        option host-name "buildvmhost-10";
	filename "pxelinux.0";
    }

    host buildvmhost-11 {
        hardware ethernet 00:25:B5:FF:00:01;
        fixed-address 10.5.125.133;
	next-server 10.5.125.43;
        option host-name "buildvmhost-11";
	filename "pxelinux.0";
    }
	 
    host buildvmhost-12 {
        hardware ethernet 00:25:B5:FF:00:05;
        fixed-address 10.5.125.134;
	next-server 10.5.125.43;
        option host-name "buildvmhost-12";
	filename "pxelinux.0";
    }

    host buildhw-01 {
        hardware ethernet e4:1f:13:78:19:6c;
        fixed-address 10.5.125.94;
        next-server 10.5.125.43;
        option host-name "buildhw-01.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host buildhw-02 {
        hardware ethernet e4:1f:13:78:0d:40;
        fixed-address 10.5.125.93;
        next-server 10.5.125.43;
        option host-name "buildhw-02.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host buildhw-03 {
        hardware ethernet E4:1F:13:78:0C:A4;
        fixed-address 10.5.125.97;
        next-server 10.5.125.43;
        option host-name "buildhw-03.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host buildhw-04 {
        hardware ethernet E4:1F:13:78:4E:80;
        fixed-address 10.5.125.95;
        next-server 10.5.125.43;
        option host-name "buildhw-04.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host buildhw-05 {
        hardware ethernet E4:1F:13:78:20:44;
        fixed-address 10.5.125.96;
        next-server 10.5.125.43;
        option host-name "buildhw-05.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host buildhw-06 {
        hardware ethernet e4:1f:13:78:38:68;
        fixed-address 10.5.125.114;
        next-server 10.5.125.43;
        option host-name "buildhw-06.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host buildhw-07 {
        hardware ethernet e4:1f:13:78:15:5c;
        fixed-address 10.5.125.115;
        next-server 10.5.125.43;
        option host-name "buildhw-07.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host buildhw-08 {
        hardware ethernet E4:1F:13:78:34:54;
        fixed-address 10.5.125.129;
        next-server 10.5.125.43;
        option host-name "buildhw-08.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host buildhw-09 {
        hardware ethernet E4:1F:13:78:0D:DC;
        fixed-address 10.5.125.130;
        next-server 10.5.125.43;
        option host-name "buildhw-09.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host buildhw-10 {
        hardware ethernet E4:1F:13:78:52:58;
        fixed-address 10.5.125.131;
        next-server 10.5.125.43;
        option host-name "buildhw-10.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host buildhw-11 {
        hardware ethernet e4:1f:13:78:19:d4;
        fixed-address 10.5.125.125;
        next-server 10.5.125.43;
        option host-name "buildhw-11.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host buildhw-12 {
        hardware ethernet E4:1F:13:78:15:40;
        fixed-address 10.5.125.126;
        next-server 10.5.125.43;
        option host-name "buildhw-12.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host x86-16 {
        hardware ethernet e4:1f:13:78:34:54;
        fixed-address 10.5.125.86;
        next-server 10.5.125.43;
        option host-name "x86-16.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

   host x86-17 {
        hardware ethernet e4:1f:13:78:0d:dc;
        fixed-address 10.5.125.87;
        next-server 10.5.125.43;
        option host-name "x86-17.phx2.fedoraproject.org";
	filename "pxelinux.0";
    }

    host x86-18 {
        hardware ethernet e4:1f:13:78:52:58;
        fixed-address 10.5.125.88;
        next-server 10.5.125.43;
        option host-name "x86-18.phx2.fedoraproject.org";
    }

    host ucs-blade01 {
        hardware ethernet 00:25:b5:ff:00:00;
        fixed-address 10.5.125.20;
        next-server 10.5.125.43;
        option host-name "ucs-blade01.phx2.fedoraproject.org";
    }

#    host x86-19 {
#        hardware ethernet e4:1f:13:78:19:d4;
#        fixed-address 10.5.125.89;
#        next-server 10.5.125.43;
#        option host-name "x86-19.phx2.fedoraproject.org";
#    }

#    host x86-20 {
#        hardware ethernet e4:1f:13:78:15:40;
#        fixed-address 10.5.125.90;
#        next-server 10.5.125.43;
#        option host-name "x86-20.phx2.fedoraproject.org";
#    }

group macs {
   allow booting;
    allow bootp;

    option domain-name "phx2.fedoraproject.org";
    option domain-name-servers 10.5.126.21, 10.5.126.22;
    option routers 10.5.125.254;

    filename "yaboot";
    authoritative;
    option dhcp-max-message-size 576;
    option dhcp-parameter-request-list = concat(
           option dhcp-parameter-request-list,
           dc, dd, e6, e8, e9, ea, eb, ec, ed, ee); # mac options

    host ppc02 {
        hardware ethernet 26:49:30:a8:7f:04;
	fixed-address 10.5.125.30;
        next-server 10.5.126.41;
        option host-name "ppc02.phx2.fedoraproject.org";
        filename "yaboot";
    }


}

#    range 10.5.125.170 10.5.125.189;
#    next-server 10.5.125.43;       
#    filename "pxelinux.0";          
}  
